**Overview**

This checklist will help you prepare for the installation of **FIT102317659.exe.**

|  |
| --- |
| General Information |
| * Product Name | Xerox® EX 280 Print Server Powered by Fiery® |
| * Current Version | 2.0 |
| * Defect ID | FIT102317659 |
| * Release Date | 16-Jul-2021 |
| * Files included | FIT102317659.exe |
| * File size | 1758521350 Bytes |
| * Checksum | 2639496 |

**Issue(s) addressed with this release**

* **FIT102317659: Fiery Patch to support Xerox Adaptive CMYK Plus.**

ImportantIcon

Before installing FIT102317659.exe

1. Known issues listed below, read before installing FIT102317659.exe patch:

* Image viewer shows separation name as Cyan, Magenta, Yellow and Black while Vivid\_kit/Fluo\_Kit workflow is in use.
* If you observe blank output when processing few files with Vivid\_kit preset and APPE enabled, please enable ‘Separate RGB/Lab to CMYK source’ from Job Properties>Color tab>Color Settings.
* Printing of files with CMYK Plus colors is supported only through Command WorkStation and not through Fiery drivers.

1. The following prerequisite(s) must be installed in the order specified before applying the FIT102317659.exe patch:

* NA

1. Do NOT install any of the following patch(es) after installing the FIT102317659.exe patch. If you must install any of the patch(es) below, do so before installing the FIT102317659.exe patch:

* None.

1. This patch is exclusive, it must be installed by itself, and the server must be rebooted or restarted once. After that, other patches can be applied to the server.
2. Patch is un-installable: Yes
3. The Fiery patch and release note have been scanned with antivirus software and believed to be virus free.

Patch installation instructions

1. Make sure that the Fiery printer controller reaches Idle.
2. Execute FIT102317659.exe and follow the instructions in the Fiery Patch Downloader.
3. Notes about the Fiery Patch Downloader
4. Login must be admin. This is fixed and cannot be modified.
5. Password is the Fiery administrator login password.
6. Hostname can be the IP address or the Fiery server name.
7. After the patch is downloaded, and when prompted by the Fiery Patch Downloader, choose Reboot now. (*If you choose to Restart later, make sure you manually reboot the server for the changes to take effect*)
8. Wait until the Fiery controller reaches Idle and print the Configuration page.
9. Verify that the **System Updates Log** section contains the patch number **FIT102317659**.